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Schonstedt Instrument Company - PRESS RELEASE

Dec. 08, 2016—for immediate publication

Contact: Wendy Hart, Marketing Director
Schonstedt’s “Maggie”: Now With Membrane Switch and IP Rating
 “Maggie”, a 2015 addition to the Schonstedt Instrument Company line of magnetic locators, has a new look and new functionality for 2017.  First, she’s gone “knobless”— a new membrane switch offers easy one-thumb operation. In addition, Maggie is now IP Rated for improved water and dust resistance ("Ingress Protection" ratings are used to define levels of sealing effectiveness of electrical enclosures against intrusion from foreign bodies and moisture).

Maggie combines the best features of two flagship products in Schonstedt’s magnetic locator line—the sensitivity and precision of the GA-52Cx, and the single-handed operation of the GA-92 XT. Says Guillermo Warley, Schonstedt’s head of engineering, “We were able to achieve an IP54 rating with this update, which is important to locators operating in harsh environments. And the membrane switch is a great enhancement to Maggie’s state-of-the-art ergonomics.”


Founded in 1953 by Erick O. Schonstedt, the company was initially a contractor to the aerospace industry, providing high-grade magnetometers for aerospace and laboratory applications. They began making magnetic locators for land surveyors in the 1970s, and the distinctive “yellow stick” soon became the global standard for survey monument location.

Call: 1-800-999-8280 / 304-725-1050 ext. 4754
Contact: Wendy Hart, Marketing Director
Click: http://www.Schonstedt.com
New Maggie images for print and Web use can be found here:

https://www.schonstedt.com/media-library/the-maggie/
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